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TT1_3rd Party Integration & Control
1) Name a Control System driver from Key Digital that can be used with CA4 and CAA?
A) Keyscan B) Compass C) Computer D) none
2) Russound has drivers available for…
A) Control 4 B) URC C) RTI D) all 3
3) Our devices communicate specifically through ___ numbers.
A) model B) controller ID C) port D) keypad
______________________________________________________________________________
TT2_Internet Music Services | No Test | Promo Only
______________________________________________________________________________
TT3_Volume Controls & Speaker Selectors
1) All Russound VC’s are ____ based.
A) resistor B) autoformer C) network D) current
2) For outdoor system applications, the ideal choice for a VC would be…
A) ALT126R B) TBL-75 C) WALTx-2 D) ALT-70V-50
3) The ALT-70V-50 wires up in ____ on the 70V speaker line.
A) series B) parallel C) stereo D) punch-down
4) Russound offers ___ different models of speaker selectors.
A) 6 B) 8 C) 11 D) 12
5) All speaker selector models include a __ year warranty.
A) 2 B) 5 C) 10 D) lifetime
_____________________________________________________________________________________
TT4_A-BUS_Multiroom Simplified
1) What type of cable run is required for an A-BUS system?
A) coax B) fiber optic C) Cat5 D) telephone
2) In an A-BUS system, the amplifier is located at the…
A) Hub B) APS Power Supply C) Keypad D) source
3) There is a _____ Out connection on the A-K4 for adding an amplifier or subwoofer.
A) Source B) Buffered C) RJ45 D) Line
4) ____ controls allow for fine-tuning L & R speaker max volume in a room.
A) zone B) input C) wireless D) gain
5) The main component that the keypads and sources are connected to is called the…
A) distribution amp B) controller C) hub D) brain
_____________________________________________________________________________
[bookmark: _Hlk498004467]TT5_WebConfig Software Tool
1) Only an authorized ___ with valid credentials can unlock gear using WebConfig. 
A) employee B) RCI C) manager D) technician
2) WebConfig is a ___ based software program.
A) IP B) browser C) controller D) 3rd party
3) WebConfig is designed to be used with your…
A) iPhone B) Android C) tablet D) all 3
4) Using WebConfig, the installer can assign…
A) zone names B) source names C) Static IP D) all 3
5) The installer should always check for the latest ___ before configuring a system
A) model number B) technology C) firmware D) system update


